IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "C:\Temp-IFC\873_0_nl_ribcassette___de_hoop_pekso_bv.ifc"
Time stamp: "2021-03-22T09:23:47"
Author: "Ronald Buitenhuis"
Organization: "De Hoop Pekso BV"
Preprocessor: "EDMsix Version 2.0100.09 Sep 7 2016"
Originating system: "Allplan 2020.1 07.07.2020 - 18:35:51"
Application: "Allplan" version "2020.1" identifier "Allplan" by Organization "De Hoop Pekso BV"

People and organizations
  Person "Ronald" "Buitenhuis" of Organization "De Hoop Pekso BV"
  Owner history of Person "Ronald" "Buitenhuis" of Organization "De Hoop Pekso BV" | application "Allplan" version "2020.1" identifier "Allplan" by Organization "De Hoop Pekso BV" | change ADDED | created 1616401426 (2021-03-22T08:23:46Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "BIM bibliotheek DHP"
  IFCBUILDING "Default Building"
    contains 8 elements
      8 x IFCBUILDINGELEMENTPROXY | names: "Isolatie Ribcassette", "Ribcassette WVR900", "Ribcassette WVR1200" (+2 more) | material: "Beton" | property sets: AllplanAttributes
    IFCBUILDINGSTOREY "Default Building Storey"

Property sets
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Isolatiewaarde (Rc-waarde in m2 K/W) = "3,5 - 4,0 - 5,0 - 6,0" (IFCDESCRIPTIVEMEASURE)
    02. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    03. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0027ErE0002311553" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "2Gw$uaulbFgAYtrnQCet9g" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "b80adc93-7a83-4745-97df-8e0530008815--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "Isolatie" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Isolatie Ribcassette" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Elementtype = "WVR 900" (IFCDESCRIPTIVEMEASURE)
    02. Lengte max. (m) = "7.00" (IFCDESCRIPTIVEMEASURE)
    03. Breedte max. (m) = "0.90" (IFCDESCRIPTIVEMEASURE)
    04. Betonkwaliteit = "C45/55" (IFCDESCRIPTIVEMEASURE)
    05. Milieuklasse = "XC, XD, XS & XF" (IFCDESCRIPTIVEMEASURE)
    06. Wapening = "Voorspanstaal Y 1860 - Betonstaal Fe 500A" (IFCDESCRIPTIVEMEASURE)
    07. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    08. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    09. Bedrijf = "De Hoop Pekso B.V." (IFCDESCRIPTIVEMEASURE)
    10. Bedrijfslocatie = "Terneuzen" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0027ErE0002311529" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "33rBX1p5zFI9K9Kjm5z10M" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "b80adc93-7a83-4745-97df-8e0530008815--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "ribcassette" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Ribcassette WVR900" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Isolatiewaarde (Rc-waarde in m2 K/W) = "3,5 - 4,0 - 5,0 - 6,0" (IFCDESCRIPTIVEMEASURE)
    02. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    03. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0030ErE0000000001" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "3X5snXVkT5Qu4P9RM0$pc1" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "8d7f4c7d-354a-4bcd-b1f2-d687dde41405--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "Isolatie" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Isolatie Ribcassette" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Elementtype = "WVR 1200" (IFCDESCRIPTIVEMEASURE)
    02. Lengte max. (m) = "7.00" (IFCDESCRIPTIVEMEASURE)
    03. Breedte max. (m) = "0.90" (IFCDESCRIPTIVEMEASURE)
    04. Betonkwaliteit = "C45/55" (IFCDESCRIPTIVEMEASURE)
    05. Milieuklasse = "XC, XD, XS & XF" (IFCDESCRIPTIVEMEASURE)
    06. Wapening = "Voorspanstaal Y 1860 - Betonstaal Fe 500A" (IFCDESCRIPTIVEMEASURE)
    07. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    08. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    09. Bedrijf = "De Hoop Pekso B.V." (IFCDESCRIPTIVEMEASURE)
    10. Bedrijfslocatie = "Terneuzen" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0030ErE0000000002" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "2tx9Ik2W964BAwI7_Re_U8" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "8d7f4c7d-354a-4bcd-b1f2-d687dde41405--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "ribcassette" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Ribcassette WVR1200" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Isolatiewaarde (Rc-waarde in m2 K/W) = "3,5 - 4,0 - 5,0 - 6,0" (IFCDESCRIPTIVEMEASURE)
    02. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    03. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0033ErE0000000002" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "0DsxYANbf6uh96ovgECqeL" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "12345b6c-891b-4471-ab23-79b67b79eaa4--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "Isolatie" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Isolatie Ribcassette" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Elementtype = "WVR 2400" (IFCDESCRIPTIVEMEASURE)
    02. Lengte max. (m) = "7.00" (IFCDESCRIPTIVEMEASURE)
    03. Breedte max. (m) = "0.90" (IFCDESCRIPTIVEMEASURE)
    04. Betonkwaliteit = "C45/55" (IFCDESCRIPTIVEMEASURE)
    05. Milieuklasse = "XC, XD, XS & XF" (IFCDESCRIPTIVEMEASURE)
    06. Wapening = "Voorspanstaal Y 1860 - Betonstaal Fe 500A" (IFCDESCRIPTIVEMEASURE)
    07. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    08. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    09. Bedrijf = "De Hoop Pekso B.V." (IFCDESCRIPTIVEMEASURE)
    10. Bedrijfslocatie = "Terneuzen" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0033ErE0000000001" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "20sOFr4nL7eQaBMeoYCroE" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "12345b6c-891b-4471-ab23-79b67b79eaa4--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "ribcassette" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Ribcassette WVR2400" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Isolatiewaarde (Rc-waarde in m2 K/W) = "4,7 - 5,0" (IFCDESCRIPTIVEMEASURE)
    02. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    03. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0035ErE0000000001" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "1Wb4woEGjElAJzZmI_GPMS" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "c345cf11-122e-4f46-bf1f-2362c0cde89b--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "Isolatie" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Isolatie Ribcassette" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    01. Elementtype = "WVR 400 (Erkerplaat)" (IFCDESCRIPTIVEMEASURE)
    02. Lengte max. (m) = "5.00" (IFCDESCRIPTIVEMEASURE)
    03. Breedte max. (m) = "0.90" (IFCDESCRIPTIVEMEASURE)
    04. Betonkwaliteit = "C45/55" (IFCDESCRIPTIVEMEASURE)
    05. Milieuklasse = "XC, XD, XS & XF" (IFCDESCRIPTIVEMEASURE)
    06. Wapening = "Voorspanstaal Y 1860 - Betonstaal Fe 500A" (IFCDESCRIPTIVEMEASURE)
    07. Fabrikant = "Waardo Beton B.V." (IFCDESCRIPTIVEMEASURE)
    08. Productielocatie = "Tiel" (IFCDESCRIPTIVEMEASURE)
    09. Bedrijf = "De Hoop Pekso B.V." (IFCDESCRIPTIVEMEASURE)
    10. Bedrijfslocatie = "Terneuzen" (IFCDESCRIPTIVEMEASURE)
    Allright_Bouwdeel_ID = "0035ErE0000000002" (IFCDESCRIPTIVEMEASURE)
    Eenheid = "m³" (IFCDESCRIPTIVEMEASURE)
    IFC-ID = "1RaKbbt1TBsALY0$2YM7QA" (IFCDESCRIPTIVEMEASURE)
    Materiaal = "Beton" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "c345cf11-122e-4f46-bf1f-2362c0cde89b--0" (IFCDESCRIPTIVEMEASURE)
    Objectnaam = "ribcassette" (IFCDESCRIPTIVEMEASURE)
    Omschrijving = "Ribcassette WVR400 (Erkerplaat)" (IFCDESCRIPTIVEMEASURE)
    Werk = "Betonwerken" (IFCDESCRIPTIVEMEASURE)